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To prevent accidental engine starting, remove.
(and isolate) spark plug leads from spark plugs
before removing gear housing.

1. Remove (and isolate) spark plug leads from
‘spark plugs.

2. Shiftengine ino forward gear:

3. Titengine o ful “Up" postion.

4. Remove fasteners.

5. Remove locknut and washer.

6. Remove gear housing.

3 - Fasteners (2 each i)
5 Lokt and Vasher




