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REMOVAL AND DISASSEMBLY

WARNING

At this step, ensure there is no spillage of

gasoline on removing the connections.

1. Remove the silencer cover, disconnect

the fuel hose, then remove the carburetor.

* Except for C60ER, C60TR, C75TR

2. Referring to the diagram, use a screwdriver

to disassemble the carburetor.

3. Using solvent, clean the components

thoroughly and blow-dry them with

compressed air.

WARNING

Protect your eyes with suitable safety

glasses or safety goggles when using compressed

air. Protect your eyes and the eyes

of others by directing the flow of compressed-

air downward, noting that solvent

and small parts may be blown off.

CAUTION:

Do not use steel wire for cleaning the jets

as this may enlarge the jet diameters and

seriously affect performance.
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1. Visually inspect the float for damage or

cracks and replace if required.

2. Measure the float height a. If it is more

than 2 mm (0.08 in) greater or less than

the specified float height, recheck the

valve seat and needle-valve.

