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INSTALLATION
1. Check that the ciutch dog shifts to “For-
ward”, “Neutral” and “"Rewverse” cor-

rectly by turning the shift rod, and shift
into “"Neutral”.

Shift rod wrench:
YB-6052

2. Align the mark on the shift lever with
the arrovw mark on the bottom cowling.

3. Grease the spline of the drive-shaft and
the water-tube outer face, align the
water-tube and drive-shaft, install the
lower unit and tighten the bolts to the
specified torque.





