[image: image1.png]7. Remove the reservoir cap @), and then
check the fluid level in the reservoir.

8. If necessary, add sufficient fluid of the
recommended type to the correct level.
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NOTE:
The fluid level should be at the brim of the
filler hole.

Recommended power trim and tilt fluid:

ATF Dexron II

9. Install the reservoir cap.

NOTE: @0
Repeat this procedure until the fluid remains
at the correct level.
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