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1. Remove the engine cover and disconnect the spark plug leads to prevent
accidental starting of the engine during lower unit removal.

2. Place a container under the gearcase. Remove the vent and drain plugs .
Drain the lubricant from the unit.

=If the lubricant is creamy in color or metallic particles are found, the
gearcase must be completely disassembled to determine and correct
the cause of the problem.

3. Wipe a small amount of ubricant on a finger and rub the finger and
thumb together. Check for the presence of mefallic particles in the lubricant. Note
the color of the ubricant. A white or creamy color indicates water in the lubricant.
Check the drain container for signs of waer separafion from the lubricant.

4. Remove the propeller as described in this chapter.

5. Place the outboard in NEUTRAL.

6. Remove the nut from the cluich shaft.

7. Disconnect the ciuteh shaft from the clutch rod.

8. Remove the bolts and lockwashers securing the gearcase to the drive-
shaft housing.

9. Remove the gearcase from the driveshaft hojing and mount it in a suit-
able hoiding fixture.

CAUTION

Do not grease the top of the driveshaft. This may excessively pre-
load the driveshaft and crankshaft when the mounting bolts are tight-
ened and cause a premature failure of the power head or gearcase.

To install:

10. Lightly lubricate the driveshaft splines and the 0-ring seal around the
driveshaft bearing with waterproof marine grease.

11. Apply a thin but uniform coat of a silicone sealer to the gearcase and
driveshaft housing mating surfaces.

12. Make sure the locating dowels are in place.
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12. Make sure the locating dowels are in place.

13. Position the gearcase under the driveshaft housing.

14. Align the driveshat splines with the crankshaft, insert the water tube into
the water pump case and the water pump seal tube.

15. Guide the clutch rod into the clutch shaft.
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8-6 LOWER UNIT

Do not rotate the flywheel counterclockwise. This can damage the
water pump impeller and cause the engine to overheat.

16. Seat the gearcase in place, rotating the flywheel clockwise as required
until the driveshaft and crankshaft engage.

17. Apply a silicone sealer to the mounting bolt threads and tighten to spec-

ifications.

18. Connect the clutch shatt onto the clutch rod and install the nut. Tighien
the nut securely.

19, Install the propeller.

20. Reconnect the spark plug leads and refill the gearcase with proper type
and quantity of lubricant. Install the engine cover.

DT75, DT85, DT115, DT140, V4 and V6 models

13. Remove the gearcase from the driveshaft housing and mount it in a suit-
able holding fixture.

Do not grease the top of the driveshaft. This may excessively pre-
load the driveshaft and crankshaft when the mounting bolts are
tightened and cause a premature failure of the power head or
gearcase.

To install:

14. Lightly lubricate the driveshatt splines with waterproof marine grease or
equivalent

15. Apply a thin but uniform coat of a sificone sealer to the gearcase and
driveshaft housing mating surfaces.

16. Make sure the locating dowels are in place.

17. Position the gearcase under the driveshaft housing.




