[image: image1.png]IMPORTANT: Use of enrichener if engine is warm
could resault in engine flooding.

[
e
G B o [ ——
R EEREEEES
]

VELTONELACK e o wre s e o 1
i )
reck it omer SLACK w3 il bock i propeny

o Vtzge ndcated
chet o open i YELLOWBLACK wre

g S Loy S (o v ) 8
Repar comectos) 3 s o key otk e "’
o e e DO N Bk gt v
FustFiow rom Fing
e G e i e
orus Pl rom Fiting

e e s e oo e
SRR A

013045-2 495

FUEL SYSTEM AND CARBURETION




