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Mercruiser 4.3L Marine Engine Performance Specifications

 (4.3L/V-6 Models)    
 

	Models 
	4.3L 
	4.3LH 
	4.3L EFI  

	Propshaft Horsepower
(SAV1 Rating)
	1901
	2051
(1902)
	2101
(1882)

	Propshaft Kilowatts
(SAV1 Rating)
	1421
	1531
(1422)
	1571
(1402)

	 Displacement
	262 cid (4.3 l)

	Maximum rpm @ WOT3
	4400-4800 rpm

	Idle rpm in NEUTRAL
	650 rpm5
	600 rpm6

	Oil Pressure @ 2000 rpm
	30-70 psi (207-483 kPa)

	Min. Oil Pressure @ Idle
	4 psi (28 kPa)

	Thermostat
	160o F (71o C)

	Timing @ Idle rpm4
	10o BTDC
	8o BTDC

	Firing Order
	1-6-5-4-3-2

	Electrical System
	12-Volt Negative (-) Ground

	Alternator Rating – Hot
Operating Amps
	65 Amps

	Alternator Rating – Cold
Operating Amps
	72 Amps

	Recommended
Battery 
Rating (Minimum)
	375 cca/
475 mca/ 90 Ah
	550 cca/
700 mca/120 Ah


1 Power Rated in Accordance with NMMA (National Marine Manufacturers’ Association) rating procedures.  
2 Power Rated in Accordance with SAV 1 rating procedures. Horsepower differences shown result from differences in test rpm, allowable test tolerances, and/or installation of special kit components.  
3 Measured using an accurate service tachometer with engine at normal operating temperature.  
4 A special procedure must be followed to check or adjust timing. Consult your Authorized mercury MerCruiser Dealer before attempting this procedure.  
5 A special procedure must be followed to adjust idle rpm. Consult your Authorized Mercury MerCruiser Dealer before attempting this procedure.  
6 Idle speed on EFI models is not adjustable. 
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