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3-19. Throttle Cam Adjustment
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motor to reach normal operating tem-

by running in a tank with test pro-
¥ in gear, at one-half throttle or slightly
before proceeding to next step.

With motor at operating temperature, run at slow
(700 - 750 rpm) with test propeller in tank or
Boat. Adjust low-speed knob until motor runs
and smoothest performance is obtained. Al

% 15 seconds for motor to respond to adjustment,

Replace low-speed valve knob with low-speed
ontrol knob in normal running position. DO NOT
disturb position of needle while installing knob.

€. With low speed needle and cam correctly ad-
Justed, motor should idle at 550 rpm IN GEAR.

FUEL PUMP
AND FILTER

Before replacing fuel pump, remove and clean the
fuel filter and install a now filter element. See
Figure 3-20. Also remove the fuel line from the fuel
fank and blow through all passages and lines with
compressed air to be sure they are open. This may
be the cause of inadequate fuel delivery, and if 8o,
would eliminate unnecessary replacement of the fuel
pump. If this procedure does not correct the trou-
Ble, fuel pump is probably malfunctioning and should
e replaced.
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Figure 3-20, Fuel Filter

TESTING FUEL PUMP

Conduct this test on the motor in a test tank or on the
boat,

1. Remove carburetor to fuel pump hose. Connect
a Iuel pressure gauge between the carburetor and
fuel pump.

NOTE

Before testing, loosen fuel fank gas cap
momentarily (o release any pressure that may
have built up. Fuel tank should not be more
than 30 inches below fuel pump.

2. Start motor and observe gauge. Pump pressures
should read as below.

R.P.M.
600 2500 to 3000 4500
1 pst L5 psI 2.5 pST

REMOVAL OF FUEL
PUMP AND FILTER

&. Disconnect hoses from pump and filter assembly.

D. To remove fuel filter, remove screw and cover
attaching filter to fuel pump. See Figure 3-20,

©. To remove fuel pump, remove two screws attach-
ing pump to power head, and remove pump assembly.
See Figure 3-20.




