[image: image1.png](3) Scrow new fiteron by hand until fier O-ring con-
tacts the mounting surfaco.

(4) Tighten iter 4 tum from point o contact with
mountng surface using an o ier wrench.

[¥) Engine ol flor: 14 N-m (1.4 kg-m, 10.0 b.1t),
.

(5) Install STBD sido covor.

6. Install gasket and ol dain plug.
Tighten engine ol drain plug o specified torque.
[¥) Engine ofl drain plug : 13 Nom (1.3 kg-m, 85 b.1t)

Do not ro-uso gaskel once romoved. Always Usoa now
gaskot.

7. Pour racommonded engine ol nto ol filr oporing, then
nstal o ilr c2p.

Engino ol amounts.
Ofl chango only :5:5 L (5.8 /4.8 US /Imp. at)
Ol fillo change :57 L (60/5.0 US /imp.at)

8 To rasat ofl change faminder systems operaton tima o

2010 (cancolaton)

(1) Tum igntion key to "ON" position.

(2) Pullout emergency stop swich pite @.

(@) Pullup smorgency stop switch knob @ threo timos in
‘soven soconds. A short boop will b hoard i cancola-
tion’s succossully finished.

&) Tum gnifon key t0"OFF” posion,then sot omergancy
stop switch piate © i orginal posiin.

NoTE:
‘520 OIL CHANGE REMINDER SYSTEM"section on page 3-22

9. Start ongine and allow i to run for sevoral minutos at ide.
spood.
‘Check ol fitr forof lskage.
“Tum off engine and waitfor appros. two minutes,then re-
check engine ol level





