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Removal of gear case
(@ Shait rod joint

The gear case can be removed without removing the power
unit from the outboard motor.
1. Remove the following:
¢ Spring pin
(Remove the spring from the upper side of gear shift
rod joint 3D.)

CAUTION

Remove the spring pin using the spring pin tool.

2. Remove the following:
¢ Gear case nuts (plain 8-4)
* Gear case assembly
(Pull out the assembly from the bottom.)

Disassembly of water pump case

@ Water pump case
® Drive shaft
® Cam rod

1. Drain the gear oil. (Refer to oil plug, Page 4-6.)
2. Remove the following:

Water pump case bolts (H652-3)

Water pump case D

Pump impeller (Pull out from the top.)

Pump impeller key

Lower pump case

Water pump assembly

@ Lower water pipe grommet
® Water pump case

® Pump case liner

@ Pump impeller

® Water pump guide plate
® Lower water pump case
@ O-ring

Pump impeller key

® Pump case bolt
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Drive shaft housing and gear case

(@ Drive shaft housing @ Propeller shaft housing
®@ Gasket Bevel gear A bearing
® Exhaust pipe ® Bevel gear C bearing
@® Gasket Needle bearing

® Gear case assembly @ Propeller shaft oil seal
® Sub-water strainer @ Oil plug





