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POWERHEAD

Water Pressure Relief Valve Components

1. If necessary, remove water pressure relief valve components as shown.

50803

1 -Cover

2 -Bolt

3 -Gasket

4 -Relief Valve Plate
5 -Diaphragm

6 - Water Deflector
7 -Washer

8 -Screw

9 -Spring

10 - Poppet Valve
11 - Grommet

12 - Carrier

13 - Washer

Torque Specifications

@150 Ib. in. (17 N'm)

®25 1b. in. (3 N-m)
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