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Water Pressure Relief Valve Components


1. If necessary, remove water pressure relief valve components as shown.
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1 - Cover
2 - Bolt
3 - Gasket
4 - Relief Valve Plate
5 - Diaphragm
6 - Water Deflector
7 - Washer
8 - Screw
9 - Spring


10 - Poppet Valve
11 - Grommet
12 - Carrier
13 - Washer


Torque Specifications


a 150 lb. in. (17 N·m)


b 25 lb. in. (3 N·m)






